# Filling the Buffer

TYPE | DIRECTIVE | OPTIONAL | ARGUMENTS
Operation | fillbuffer | Yes | <data>

The fillbuffer directive is used to initialize the buffer with the specified value.

The buffer is filled in the address range defined by the last addrange directive.

<data> = value used to reset the buffer; may be written in decimal or hexadecimal format.

Example of use :

> batchisp -device t89c51cc01 -hardware PEAK -operation memory FLASH fillbuffer 0x00 memory EEPROM fillbuffer 0xFF