# Setting the AutoISP Mode

TYPE | SWITCH | OPTIONAL | ARGUMENTS
Setup | -autoisp | Yes | { 0 | 1 } { 0 | 1 }

Example of use :

> batchisp -device at89c51rd2 -autoisp -operation erase F -demo

The -autoisp switch may have two arguments or no argument at all; there is no other possible number of arguments.

The first argument is the RESET signal active level. The second argument is the PSEN signal active level.

With the above command line, batchisp displays the following :