Operations Directives Summary

# Operation Directives Summary

Operations directives are arguments of the -operation switch; they are not case sensitive.

Values in bold in the arguments lists are default ones.

Opening a CAN Node

Closing a CAN Node

Selecting the Target Memory

Specifying a Range of Addresses

Erasing Memory

Blank Checking Memory

Loading the ISP Buffer

Filling the Buffer

Programming Memory

Verifying Memory

Reading Memory

Saving the Buffer Contents to a File

Serializing Parts

Launching the Embedded Application

Inserting Wait States

Reading and Writing Special Bits and Bytes

Changing the On Fail Behavior

Asserting Operation Results