INSTALL - FLIP
               

Atmel


Requirements
------------

This program runs on Windows 98/Me/NT/2000/XP.


Windows Installation
--------------------

- Copy the Flip_<version>.zip file to an empty temporary directory.
- Uncompress the zip file so that you get a Flip_<version> directory.
- Open the Flip_<version> directory and run the Setup file.
- Follow the installation program instructions.


Post Installation Instructions
------------------------------

CAN

After FLIP installation completion, CAN users must install their
CAN dongle software and reboot their PC platform.

The VECTOR CANpari dongle requires the user's PATH variable 
to be updated so that it contains the path to the vccand32.dll file.

Before using the PEAK PCAN dongle, you must launch the PEAK dll
installation program named pcandrv.exe and located in the 
<your_HDD>:\Program Files\ATMEL\FLIP x.y.z


USB

After FLIP installation completion, USB users must execute
Start > Programs > Atmel > FLIP x.y.z > Install USB Drivers

FLIP-USB can be used on Windows 98/Me/2000/XP platforms only.


